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Quotation

	MODEL
	QUANTITY
	PRICE-FOB SHANGHAI

	Washing label printer
	1 SET
	USD 21000/SET

	INK 
	1 SET
	USD 75/SET

	Cleaner
	[bookmark: _GoBack]1 BOTTLE
	USD 35/BOTTLE

	Printer head
	1 PCS
	USD 1200/PCS

	· Terms of Payment:
[bookmark: OLE_LINK1]   30% deposit by T T when confirming the order
	70% balance by T T before shipping.
   Or irrevocable L C at sight
· Installation and Training
   The price includes the fee of installation, Training and interpreter, However,
   the relative cost such as international air tickets between China and 
   Buyer’s country, local transportation, accommodation (3 star hotel), and the    
   pocket money USD90 day per person for engineers and interpreter will be  
   born by buyer. Or, the customer can find capable interpreter in local.
· Validity of Quotation
   Until 30th Dec. 2025
· Warranty
   12 months after B L date
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Digital Printing And Label Cutting
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Standard Edition

Printing Width:0-67.6mm

Printing Epeedﬂ -A0m/min * This machine is suitable for various wash-
' resistant inkjet coated substrates, including

Printing resolution:600-1200dpi coated, satin, polyester, hemmed, tear-away

« and cotton tapes, as well as colorful gift
Ink color:CMYK packaging woven ribbons. Paired with special

Size:1141.8*649.6*1165.4mm wash-resistant CMYK four-color inks,

Voltage:2kw « Besides narrow-width fabric tapes, it also

_ : supports ordinary paper, synthetic paper,
Printhead options: glossy paper, matte paper and films, satisfying
EPSON 13200-A1 users' diversified label printing needs.

EPSON I13200-A1THD
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Pro Edition

Printing Width:0-67.6mm
Printing speed:1-40m/min
Printing resolution:600-1200dpi
Ink color:CMYK
Size:1141.8"649.6"1165.4mm
Voltage:2kw

Printhead options:

EPSON I3200-A1

EPSON I3200-A1THD

This advanced model is designed for mid-to-
high volume label production and professional
processing factories.

It retains the standard version’ s full substrate
compatibility for wash-resistant fabric tapes
and woven ribbons, with improved printing
speed and precision. Featuring an optimized
mechanical structure and ink supply system, it
ensures stable high-quality output during long-
hour continuous operation.

It supports thicker and special-shaped media,
and is equipped with intelligent media
detection and automatic tension control, ideal
for apparel wash-care labels, industrial tags,
high-end gift packaging ribbons and other
complex label applications.
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Dual-Head Printing Edition

Printing Width:0-67.6mm * This high-efficiency model is designed for
large-scale production lines and high-

Printing speed:1-40m/min demand label processors.

Printing resolution:600-1200dpi , Equipped with dual independent print heads,

Ink color:CMYK it enables support double-sided printing.,
greatly improving productivity while

Size:1150*630*1350mm maintaining full compatibility with wash-
resistant substrates and woven ribbons. The

Voltage:2kw dual-head design ensures stable high quality.

Printhead options: « Supporting fabric tapes, papers and films, it

EPSON 13200-A1 features automatic head alignment, real-time
ink monitoring and batch processing, making
EPSON I13200-A1HD it an ideal solution for high-efficiency, high-

quality large-volume label production.
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Appliactions
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The Advantages Of 13200A1 and 13200A1HD

1200 dpi

2 colors * High-Speed Efficiency
..+.o» e Superior Print Precision

e Vivid Color Performance

High density Printhead

e Durable & Versatile Design
EPSON-13200A1 EPSON-I3200A1HD

Flexible Configuration &

Compatibility

ML X0
| . UPGJET

SHANGHAI UPG DIGITAL TECHNOLOGY CO.LTD.

ROOM 2201, HENGHUI BUILDING, NO. 568, HENGFENG ROAD,
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ADVANTAGES FOR DIGITAL
PRINTING MACHINE

Traditional Printing And Label Cutting
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